=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Jul-2012
Following new information from the data suppliers, KHOA the values for lat.
and long. for this station have been revised.
Tide gauge is an OTT float gauge
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 16-Apr-2026
Updated the entire dataset to L2 dataset to ensure users can access fully quality-controlled sea level data for long-term variability and trend analysis.

