=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Anhung              620/014 RLR(1989) is 14.4m below TBM No 1
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jul-1993
Anhung              620/014 RLR(1989) is 14.4m below TBM No 1
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 08-Dec-1997
Type of tide gauge: OTT float type
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 08-Dec-2010
Primary benchmark 1989-1990 is TBM No.1. From 1991 onwards Primary benchmark is
TBM No.3. Datum TGZ remains the same throughout.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Jul-2012
At the request of the supplying authority, KHOA the name for this station has
been changed to Anheung. The latitude and longitude have also been revised.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 16-Apr-2026
Updated the entire dataset to L2 dataset to ensure users can access fully quality-controlled sea level data for long-term variability and trend analysis.

