=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Wando               620/034 RLR(1984) is 10.0m below TBM No2
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jul-1993
Wando               620/034 RLR(1984) is 10.0m below TBM No2
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 08-Dec-1997
Type of tide gauge: OTT float
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Jul-2012
Following receipt of new information from the data suppliers, KHOA the values
of lat. and long. have been revised.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 16-Apr-2026
Updated the entire dataset to L2 dataset to ensure users can access fully quality-controlled sea level data for long-term variability and trend analysis.

