=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Chujado             620/039 RLR(1985) is 12.4m below TBM No2
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jul-1993
Chujado             620/039 RLR(1985) is 12.6m below TBM No2
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 08-Dec-1997
Type of tide gauge: OTT float
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Jul-2012
Following information received from the supplying authority, KHOA the lat.
and long. have been revised.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 16-Apr-2026
Updated the entire dataset to L2 dataset to ensure users can access fully quality-controlled sea level data for long-term variability and trend analysis.

