=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Sogwipo             620/032 RLR(1986) is 10.4m below TBM No2
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jul-1993
Sogwipo             620/032 RLR(1986) is 10.4m below TBM No2
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 08-Dec-1997
Type of tide gauge: OTT float
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Jul-2012
At the request of the data suppliers, KHOA the name of this station has
been revised to Seogwipo. The values of lat. and long. have also been revised.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 16-Apr-2026
Updated the entire dataset to L2 dataset to ensure users can access fully quality-controlled sea level data for long-term variability and trend analysis.

