=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Pusan               620/046 RLR(1963) is 8.9m below TBM no.1
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 26-Feb-1993
gauge resited 1973
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Jul-1993
Pusan               620/046 RLR(1963) is 8.9m below TBM no.1
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 08-Dec-1997
Type of tide gauge: OTT float
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Jul-2012
At the request of the supplying authority, KHOA the name has been changed to
read Busan the lat. and long. have also been revised.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 16-Apr-2026
Updated the entire dataset to L2 dataset to ensure users can access fully quality-controlled sea level data for long-term variability and trend analysis.

