=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Jun-1991
Yosu                620/036 RLR(1966) is 11.1m below TBM No2
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Jul-2012
At the request of the data supplier, KHOA the name of this station has been
changed to Yeosu. The values for lat. and long, have also been revised.
Tide gauge is a MIROS radar gauge
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 15-Aug-2012
When preparing the RLR diagram to be displayed on the PSMSL website it was
noted that the data for 1966-1969 was not RLR. There are no problems with
the data for this period so the whole dataset 1966 onwards is now RLR.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 16-Apr-2026
Updated the entire dataset to L2 dataset to ensure users can access fully quality-controlled sea level data for long-term variability and trend analysis.

